# geometry of blind defined in: ../zones/blind.geo
GEN  blind  blind describes the external blind  # type, name, descr
       8       6   0.000    # vertices, surfaces, rotation angle
#  X co-ord, Y co-ord, Z co-ord
      0.68652    -0.57949     0.46000  # vert   1
      1.70949    -1.14653     0.46000  # vert   2
      1.70949    -1.14653     1.88000  # vert   3
      0.68652    -0.57949     1.88000  # vert   4
      0.76409    -0.41452     0.46000  # vert   5
      1.78706    -0.98152     0.46000  # vert   6
      1.78706    -0.98152     1.88000  # vert   7
      0.76409    -0.41452     1.88000  # vert   8
# no of vertices followed by list of associated vert
   4,  1,  2,  3,  4,
   4,  2,  6,  7,  3,
   4,  6,  5,  8,  7,
   4,  5,  1,  4,  8,
   4,  4,  3,  7,  8,
   4,  1,  5,  6,  2,
# unused index
 0,0,0,0,0,0
# surfaces indentation (m)
 0.00,0.00,0.00,0.00,0.00,0.00
    1   3   0   3    # default insolation distribution
# surface attributes follow: 
# id  surface      geom  loc/  construction environment
# no  name         type  posn  name         other side
  1, window        TRAN  VERT  glazing      EXTERIOR       
  2, Surf-2        OPAQ  VERT  insulation   ADIABATIC      
  3, Surf-3        TRAN  VERT  shade        cell           
  4, Surf-4        OPAQ  VERT  insulation   ADIABATIC      
  5, Surf-5        OPAQ  CEIL  insulation   ADIABATIC      
  6, Surf-6        OPAQ  FLOR  insulation   ADIABATIC      
# base
  6  0  0  0  0  0     0.21 2
