# geometry of blind defined in: ../zones/blind.geo
GEN  blind  blind describes the external blind  # type, name, descr
       8       6   0.000    # vertices, surfaces, rotation angle
#  X co-ord, Y co-ord, Z co-ord
      0.68652    -0.51949     0.46000  # vert   1
      1.70949    -1.08653     0.46000  # vert   2
      1.70949    -1.08653     1.88000  # vert   3
      0.68652    -0.51949     1.88000  # vert   4
      0.73500    -0.40700     0.46000  # vert   5
      1.75797    -0.97400     0.46000  # vert   6
      1.75797    -0.97400     1.88000  # vert   7
      0.73500    -0.40700     1.88000  # vert   8
# no of vertices followed by list of associated vert
   4,  1,  2,  3,  4,
   4,  2,  6,  7,  3,
   4,  6,  5,  8,  7,
   4,  5,  1,  4,  8,
   4,  4,  3,  7,  8,
   4,  1,  5,  6,  2,
# unused index
 0,0,0,0,0,0
# surfaces indentation (m)
 0.00,0.00,0.00,0.00,0.00,0.00
    1   3   0   3    # default insolation distribution
# surface attributes follow: 
# id  surface      geom  loc/  construction environment
# no  name         type  posn  name         other side
  1, Surf-1        TRAN  VERT  shade        EXTERIOR       
  2, Surf-2        TRAN  VERT  fictitious   ADIABATIC      
  3, Surf-3        TRAN  VERT  glazing      cell           
  4, Surf-4        TRAN  VERT  fictitious   ADIABATIC      
  5, Surf-5        TRAN  CEIL  fictitious   ADIABATIC      
  6, Surf-6        TRAN  FLOR  fictitious   ADIABATIC      
# base
  6  3  0  0  0  0     1.80 0
