proj cntrl  # overall descr
* Building
no descrip  # bld descr 
   7  # No. of functions
* Control function
# senses dry bulb temperature in cell.
    1    0    0    0  # sensor data
# actuates the air point in cell.
    1    0    0  # actuator data
    1 # No. day types
    1  365  # valid Thu  1 Jan - Fri 31 Dec
     1  # No. of periods in day
    0    2   0.000  # ctl type, law (free floating), start @
      0.  # No. of data items
* Control function
# reads measurements from a boundry data file. 1
   -5    1    0    0  # sensor data
# actuates the air point in west_zone.
    2    0    0  # actuator data
    1 # No. day types
    1  365  # valid Thu  1 Jan - Fri 31 Dec
     1  # No. of periods in day
    0   11   0.000  # ctl type, law (match temp - ideal), start @
     10.  # No. of data items
  10000.000 0.000 10000.000 0.000 1.000 1.000 -5.000 0.000 0.000 0.000
* Control function
# reads measurements from a boundry data file. 1
   -5    1    0    0  # sensor data
# actuates the air point in east_zone.
    3    0    0  # actuator data
    1 # No. day types
    1  365  # valid Thu  1 Jan - Fri 31 Dec
     1  # No. of periods in day
    0   11   0.000  # ctl type, law (match temp - ideal), start @
     10.  # No. of data items
  10000.000 0.000 10000.000 0.000 1.000 1.000 -5.000 0.000 0.000 0.000
* Control function
# reads measurements from a boundry data file. 1
   -5    1    0    0  # sensor data
# actuates the air point in top_zone.
    4    0    0  # actuator data
    1 # No. day types
    1  365  # valid Thu  1 Jan - Fri 31 Dec
     1  # No. of periods in day
    0   11   0.000  # ctl type, law (match temp - ideal), start @
     10.  # No. of data items
  10000.000 0.000 10000.000 0.000 1.000 1.000 -5.000 0.000 0.000 0.000
* Control function
# reads measurements from a boundry data file. 1
   -5    1    0    0  # sensor data
# actuates the air point in base_zone.
    5    0    0  # actuator data
    1 # No. day types
    1  365  # valid Thu  1 Jan - Fri 31 Dec
     1  # No. of periods in day
    0   11   0.000  # ctl type, law (match temp - ideal), start @
     10.  # No. of data items
  10000.000 0.000 10000.000 0.000 1.000 1.000 -5.000 0.000 0.000 0.000
* Control function
# reads measurements from a boundry data file. 1
   -5    1    0    0  # sensor data
# actuates the air point in north_zone.
    6    0    0  # actuator data
    1 # No. day types
    1  365  # valid Thu  1 Jan - Fri 31 Dec
     1  # No. of periods in day
    0   11   0.000  # ctl type, law (match temp - ideal), start @
     10.  # No. of data items
  10000.000 0.000 10000.000 0.000 1.000 1.000 -5.000 0.000 0.000 0.000
* Control function
# reads measurements from a boundry data file. 1
   -5    1    0    0  # sensor data
# actuates the air point in south_zone.
    7    0    0  # actuator data
    1 # No. day types
    1  365  # valid Thu  1 Jan - Fri 31 Dec
     1  # No. of periods in day
    0   11   0.000  # ctl type, law (match temp - ideal), start @
     10.  # No. of data items
  10000.000 0.000 10000.000 0.000 1.000 1.000 -5.000 0.000 0.000 0.000
# Function:Zone links
 1,2,3,4,5,6,7
