# geometry of base_zone defined in: ../zones/base_zone.geo
GEN  base_zone  base guard zone  # type, name, descr
      12       8   0.000    # vertices, surfaces, rotation angle
#  X co-ord, Y co-ord, Z co-ord
      0.00000     0.00000    -1.00000  # vert   1
      2.85000     0.00000    -1.00000  # vert   2
      2.85000     9.98000    -1.00000  # vert   3
      0.00000     4.62600    -1.00000  # vert   4
      0.00000     0.00000     0.00000  # vert   5
      2.85000     0.00000     0.00000  # vert   6
      2.85000     9.98000     0.00000  # vert   7
      0.00000     4.62600     0.00000  # vert   8
      2.80000     4.62600    -1.00000  # vert   9
      2.80000     4.62600     0.00000  # vert  10
      2.80000     9.98000    -1.00000  # vert  11
      2.80000     9.98000     0.00000  # vert  12
# no of vertices followed by list of associated vert
   4,  1,  2,  6,  5,
   4,  2,  3,  7,  6,
   4,  9,  4,  8, 10,
   4,  4,  1,  5,  8,
   6,  5,  6,  7, 12, 10,  8,
   6,  1,  4,  9, 11,  3,  2,
   4, 11,  9, 10, 12,
   4,  3, 11, 12,  7,
# unused index
 0,0,0,0,0,0,0,0
# surfaces indentation (m)
 0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00
    3   0   0   0    # default insolation distribution
# surface attributes follow: 
# id  surface      geom  loc/  construction environment
# no  name         type  posn  name         other side
  1, Surf-1        OPAQ  VERT  intwall      SIMILAR        
  2, Surf-2        OPAQ  VERT  intwall      SIMILAR        
  3, Surf-3        OPAQ  VERT  intwall      SIMILAR        
  4, Surf-4        OPAQ  VERT  intwall      SIMILAR        
  5, base          OPAQ  CEIL  floor_inv    cell           
  6, Surf-6        OPAQ  FLOR  intwall      SIMILAR        
  7, Surf-7        OPAQ  VERT  intwall      SIMILAR        
  8, Surf-8        OPAQ  VERT  intwall      SIMILAR        
# base
  6  0  0  0  0  0    13.45 0
