# geometry of south_zone defined in: ../zones/south_zone.geo
GEN  south_zone  south guard zone  # type, name, descr
       8       6   0.000    # vertices, surfaces, rotation angle
#  X co-ord, Y co-ord, Z co-ord
      0.00000    -1.00000     0.00000  # vert   1
      2.85000    -1.00000     0.00000  # vert   2
      2.85000     0.00000     0.00000  # vert   3
      0.00000     0.00000     0.00000  # vert   4
      0.00000    -1.00000     2.36000  # vert   5
      2.85000    -1.00000     2.36000  # vert   6
      2.85000     0.00000     2.36000  # vert   7
      0.00000     0.00000     2.36000  # vert   8
# no of vertices followed by list of associated vert
   4,  1,  2,  6,  5,
   4,  2,  3,  7,  6,
   4,  3,  4,  8,  7,
   4,  4,  1,  5,  8,
   4,  5,  6,  7,  8,
   4,  1,  4,  3,  2,
# unused index
 0,0,0,0,0,0
# surfaces indentation (m)
 0.00,0.00,0.00,0.00,0.00,0.00
    3   0   0   0    # default insolation distribution
# surface attributes follow: 
# id  surface      geom  loc/  construction environment
# no  name         type  posn  name         other side
  1, Surf-1        OPAQ  VERT  southwall    EXTERIOR       
  2, Surf-2        OPAQ  VERT  southwall    SIMILAR        
  3, south         OPAQ  VERT  southwall    cell           
  4, Surf-4        OPAQ  VERT  southwall    SIMILAR        
  5, Surf-5        OPAQ  CEIL  southwall    SIMILAR        
  6, Surf-6        OPAQ  FLOR  southwall    SIMILAR        
# base
  6  0  0  0  0  0     2.85 0
